(footprint "Relay_DPDT_Panasonic_TQ2-SA"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Panasonic TQ2-SA SMD DPDT (2 Form C) signal relay, 10 SMD terminals. Land pattern derived from the Panasonic TQ-SMD datasheet 'Recommendable mounting pad (Top view), SA type': 2.54mm row pitch, pad 1.0 x 2.94 mm, two rows at +/-3.31mm (9.56mm outer span), ~14mm overall. Pin map: coil 1/10; pole1 COM=3 NC=4 NO=2; pole2 COM=8 NC=7 NO=9. VERIFY against the datasheet before fab.")
	(tags "relay Panasonic TQ2 TQ2SA DPDT 2FormC SMD")
	(property "Reference" "REF**"
		(at 0 -6 0)
		(layer "F.SilkS")
		(uuid "20e13ea2-2257-4b4a-a53e-9d3c94dd6bb3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "TQ2SA-5V"
		(at 0 6 0)
		(layer "F.Fab")
		(uuid "58c051b0-2d2f-4a32-a1f7-505512d81218")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://industrial.panasonic.com/ww/products/pt/tq"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "5c67e25e-81d3-445b-97d2-43119d6e39dc")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Panasonic TQ2-SA DPDT signal relay"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "20a952d1-ff72-4879-bd1e-80e5859d208e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -7 -4.5)
		(end 7 -4.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "d886079d-cdaf-475c-8aa7-32035c18a226")
	)
	(fp_line
		(start -7 4.5)
		(end 7 4.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "2647f0ce-0b5c-4f5e-b966-d3f873b32ad4")
	)
	(fp_circle
		(center -6.5 -4)
		(end -6.3 -4)
		(stroke
			(width 0.2)
			(type default)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "dec3a367-3d98-4060-be90-e5a7bf5854c9")
	)
	(fp_rect
		(start -7.7 -5.4)
		(end 7.7 5.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "d6a2930d-0aca-41af-87a6-a0e76f97e85a")
	)
	(fp_rect
		(start -7 -4.5)
		(end 7 4.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "82dbbeab-fe2f-4ee0-be6c-14536513b34d")
	)
	(pad "1" smd roundrect
		(at -5.08 -3.31)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "8b24d11a-e344-417e-a739-9aa09d9d668f")
	)
	(pad "2" smd roundrect
		(at -2.54 -3.31)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "2e7e36aa-115d-4b44-bcd0-a8aa0e78ff00")
	)
	(pad "3" smd roundrect
		(at 0 -3.31)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "2bca0a65-ef27-4bd0-872a-0ffaa70634d9")
	)
	(pad "4" smd roundrect
		(at 2.54 -3.31)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "c6bde6c3-ed9a-4374-bc5d-007be9adb4d5")
	)
	(pad "5" smd roundrect
		(at 5.08 -3.31)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "9e38c1e9-6197-4cc6-b7a2-8b4c5261fead")
	)
	(pad "6" smd roundrect
		(at 5.08 3.31)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "af54b502-62f4-4ad4-a150-c038f527dcb7")
	)
	(pad "7" smd roundrect
		(at 2.54 3.31)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "3f57f831-9d5c-4052-a9af-53c2fdee994f")
	)
	(pad "8" smd roundrect
		(at 0 3.31)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "b3a87d9e-357b-4685-a78b-8b23e0bb20ad")
	)
	(pad "9" smd roundrect
		(at -2.54 3.31)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "5147e9ac-2ddd-4ed1-9ba7-b0da686c5cc3")
	)
	(pad "10" smd roundrect
		(at -5.08 3.31)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "1d45a9c4-d273-4376-8f72-d26b07458648")
	)
	(embedded_fonts no)
)
