(footprint "RV-8803-C7"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Micro Crystal RV-8803-C7 I2C RTC, SON-8 ceramic 3.2x1.5x0.8mm. Land pattern from the datasheet (doc RV-8803-C7, Mouser 2308195) Recommended Solder Pad: pad 0.4 x 0.8 mm, pitch 0.9 mm (X), two rows 0.5mm inner gap -> 1.3mm center-to-center (rows +/-0.65mm). Top-view pin map (pin-1 index bottom-left): bottom L->R = 1,2,3,4 ; top L->R = 8,7,6,5. 1=SDA 2=CLKOUT 3=VDD 4=CLKOE 5=VSS 6=/INT 7=EVI 8=SCL. VERIFY the 0.4/0.8/0.9/0.5 numbers against the drawing.")
	(tags "RTC I2C MicroCrystal RV-8803 SON-8")
	(property "Reference" "REF**"
		(at 0 -1.6 0)
		(layer "F.SilkS")
		(uuid "db94bdc4-f491-4d1a-a0f6-2af3485c7953")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.12)
			)
		)
	)
	(property "Value" "RV-8803-C7"
		(at 0 1.6 0)
		(layer "F.Fab")
		(uuid "8b098e33-fbac-4a8d-9196-9768322b4f49")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.12)
			)
		)
	)
	(property "Datasheet" "https://www.microcrystal.com/fileadmin/Media/Products/RTC/Datasheet/RV-8803-C7.pdf"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "70208115-007d-4854-82ab-38a363d72138")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.1)
			)
		)
	)
	(property "Description" "Micro Crystal RV-8803-C7 I2C RTC, SON-8"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "d186185c-5fb4-4f14-84da-c51bb56fb4be")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.1)
			)
		)
	)
	(attr smd)
	(fp_circle
		(center -1.85 1)
		(end -1.75 1)
		(stroke
			(width 0.15)
			(type default)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "72c1c634-b952-418f-af45-674e2220124d")
	)
	(fp_rect
		(start -1.9 -1.15)
		(end 1.9 1.15)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "62649bd7-29b7-4b2d-9b36-cc43829314af")
	)
	(fp_rect
		(start -1.6 -0.75)
		(end 1.6 0.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "cacaa345-30e2-43b2-854f-ae63f1669346")
	)
	(pad "1" smd roundrect
		(at -1.35 0.65)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "dcf9769c-71d8-41d3-81cd-dc7b0a77da0d")
	)
	(pad "2" smd roundrect
		(at -0.45 0.65)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "bdb930da-5abe-44cc-9a15-21573286262c")
	)
	(pad "3" smd roundrect
		(at 0.45 0.65)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "ed65728b-1ce6-4553-b02b-60d6e2012701")
	)
	(pad "4" smd roundrect
		(at 1.35 0.65)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "7ddbefdc-3020-4f5b-8d4e-7f35628b4b77")
	)
	(pad "5" smd roundrect
		(at 1.35 -0.65)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "fc535879-d6bb-4506-927a-86017e48e026")
	)
	(pad "6" smd roundrect
		(at 0.45 -0.65)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "a9cea043-d14e-48e5-b2ff-eb0152772c9d")
	)
	(pad "7" smd roundrect
		(at -0.45 -0.65)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "8e50f635-2d1e-44a1-874a-f7b26f11fe9e")
	)
	(pad "8" smd roundrect
		(at -1.35 -0.65)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "9142efa1-e0f4-403e-abcc-ce468d17eeab")
	)
	(embedded_fonts no)
)
